# IxB Tools restrictions

## IxB connect functionality requirements

The IxB connect functionality requires:

- PF6000 controller from version 13 and above

- PF8 controller revision 5 and above

## Maximum number of tool connections

Controller | Connectivity type | IxB tool no. of tools | IxB and other wireless tools no. of tools
--- | --- | --- | ---
PF6000 | Wireless LAN | 6 | 6 (no matter the combination)
Bluetooth supported tools = IxB/XB tools only | 4 | NA
Bluetooth supported tools = No IXB/XB tools | 0 | 6 wireless tools
PF8 | Wireless LAN | 20 | 20
Bluetooth | 6 | 6 (no matter the combination)