# TAG Selection

TAG selection feature is used for selecting a Tightening Program/Batch or Batch Sequence that has a TAG number configured that corresponds to the TAG number of the TAG inserted into the STwrench smartHEAD.

TAG selection is available only for STwrench.

TAG selection options | Description
--- | ---
Off | The STwrench does not signal the controller to select Tightening Program/Batch or Batch Sequence.
On | Select the Tightening Program/Batch or Batch Sequence according to the TAG number configured in the Batch Sequence/Source Tightening/Source Batch.