# Configuring the storage of Final Torque and Trace

The switch Store with PrT compensation is by default set to ON which means that the final torque and trace are stored with the PrT compensation value.
Show Final Torque with PrT compensation in the Live Result Presentation Settings determines what is shown in Live result.

## Changing the Store with PrT compensation setting

1. On the home view, select Configurations.

2. Scroll down and select General Virtual Station on the left pane.

3. In the Configuration window, select a Configuration and then Edit. The Edit configuration window appears.

4. Scroll down to Storage of Final torque and Trace, set the switch Store with PrT compensation into the wanted position.