# Configuring Live Result Presentation Settings

The Live Result Presentation Settings window allows a user to show the final torque without the PrT compensation value included, and PrT compensation value on the Live results.

## Configure the Live Result Presentation Settings Window

1. On the home view, go to the Configurations tab and select General Virtual Station on the left pane.

2. On the Configuration window you want to work with, select Edit.
   The Edit Configuration screen appears.

3. On the Live Result Presentation Settings window, set the relevant switches to ON or OFF depending on the wanted results.

   If the Show PrT Compensation Value switch is set to ON, the Live Results window displays the PrT compensation value.

   If the Show Final Torque with PrT Compensation switch is set to ON, the Live Results window displays the final torque with the PrT compensation included.

   Setting the switches in the Live Results Presentations Settings window to either ON or OFF has no impact unless the multistep program has a tightening step including a Prevailing Torque step monitor with the Compensation switch set to ON.

## Live Result Presentation Settings

Here are the different configuration options in the Live Results Presentations Settings window.

Show PrT Compensation Value: ON Show Final Torque with PrT Compensation: ON | Show PrT Compensation Value: ON Show Final Torque with PrT Compensation: OFF | Show PrT Compensation Value: OFF Show Final Torque with PrT Compensation: ON | Show PrT Compensation Value: OFF Show Final Torque with PrT Compensation: OFF
--- | --- | --- | ---
Point and click on image to see more information: | Point and click on image to see more information: | Point and click on image to see more information: | Point and click on image to see more information:

In this Section

- Show Final Torque with PrT Compensation: ON / Show PrT Compensation Value: ON
- Show Final Torque with PrT Compensation: OFF / Show PrT Compensation Value: ON
- Show Final Torque with PrT Compensation: OFF / Show PrT Compensation Value: OFF
- Show Final Torque with PrT Compensation: ON / Show PrT Compensation Value: OFF