# Show Final Torque with PrT Compensation: ON / Show PrT Compensation Value: ON

## Show Final Torque with PrT Compensation: ON

The Live Result window shows the Final Torque with the PrT compensation value included.

If the EHMI and ST Selector are on and configured, they show the Final Torque with the PrT compensation value included.

## Show PrT Compensation Value on Live Result: ON

The Live Result window shows the PrT compensation value with the related compensation icon ().

If there are several compensation values, the compensation value applied to the latest available step appears.

Configuring the Show Final Torque with PrT Compensation and Show PrT Compensation Value switches does not impact:

- The final torque values sent to ToolsNet and ToolsTalk: the final torque values with PrT compensation are always sent to ToolsNet and ToolsTalk.

- The final torque value displayed with the historical results.

- The traces based on live and historical results.

- The values in Open Protocol messages.

- The signals.

- The protocol adapters.