# Assembling the Panel PC

- Only qualified personnel shall assemble and operate the Panel PC.

- Only suspended or standing assembly with standard screen of the Panel PC is permitted. Vertical screen orientation is not permitted.

Assemble the Panel PC as follows:

1. Partly install the two bottom screws first. The original size of these screws is 4x M4x10mm with 4x M4 washer included in Part Number 8434230430 AC Mini vesa adapter.