# Configuring a Source Tightening

1. Go to Sources in the home menu, and select Tightening in the left pane.

2. Select the plus icon in the top right.

3. Issue the source tightening with a Name and select the correct Selector mode (Control or Confirm, depending on what is required).

4. Max consecutive NOK can be set per source tightening or per individual program included in the source tightening. Set Max consecutive NOK per program parameter to Yes or No, depending on what is required:

   - To set the max consecutive NOK per source tightening, set Max consecutive NOK per program to No. Set the value in the Max consecutive NOK field.

   - To set the max consecutive NOK per program, set Max consecutive NOK per program to Yes. For every program in the Identifier selector configuration section, set the value in the Max NOK column.

5. Barcode Required can be set per source tightening or per individual program included in the source tightening.

   - To set the Barcode Required per source tightening, set Barcode Required to Yes. A barcode scan will be required in order to start each program in the source tightening.

   - To set the Barcode Required per program, set Barcode Required to Yes. Then, for each program in the Identifier selector configuration section, select No or Yes in the Barcode Required column to respectively disable or enable the barcode required feature for the individual program.

6. By default, only one editable identifier number will be available when creating a new source tightening. At the bottom of the screen, select the plus icon to add more.

7. Give every item an identifier number.

   To activate the program, the identifier number linked to the tightening program must correspond to the ID sent with the external digital signal (Open protocol).

   If Confirm mode is selected as Selector Mode, type an additional identifier under the Socket Identifier column for the end fitting tool (TAG) or socket to be used for the tightening program (max. value: 32).

8. Choose a tightening program to link to each identifier number by selecting a row and choosing from the list of tightening programs.