# Live Results View

The Live Results page is available only when the STRwrench is working with the Integrated Controller Tool.

In the bottom bar of the STRwrench Web User Interface, click the results icon () to open the Live Results page:

Position | Description
--- | ---
1 | Target torque.
2 | Torque result.
3 | Angle result.
4 | Target angle.
5 | Result status.
6 | A NOK tightening will give a detailed status of the unsuccessful tightening.
7 | VIN (Vehicle identification number) scanned by the barcode reader.
8 | Amount of time passed between the start and the end of the tightening.
9 | Number of completed batches in the sequence.
10 | Batch sequence name.
11 | Total number of batches in the sequence.
12 | Result of each completed batch in the sequence: An ongoing batch is colored white. An OK batch is colored gray, with the number boxed. A NOK batch is colored red, with the number boxed and crossed out.
13 | Number of completed tightenings in the batch.
14 | Tightening program name.
15 | Total number of tightenings in the batch.
16 | Number of completed tightenings in the batch: An OK tightening is colored gray, with the number circled. A NOK tightening is colored red, with the number circled and crossed out.

Click the arrows on both sides of the page to change view and display the graph of the ongoing tightening.

If you leave the Live Results page, the live results session ends and data is cleared.