# Tightening Program Library - Updating a Global Tightening Program

1. Select Library in the left-side menu bar.

2. Go to Tightening Program .

   The workspace area shows a list of Global tightening programs.

3. Double-click on the name field, the tightening menus are editable. The changes are auto saved to the tightening program.

A global tightening program can only be edited or updated if the tightening menus are opened via the library path.

WARNING

Risk of injury

A change in configuration to the tightening program may cause unexpected torque, rotational direction, or speed in the system(s) where the tightening program is currently in use. This could result in severe bodily injury and/or property damage.

- Check the tightening program configurations after adding a new program or after applying changes to an existing program.

Updates to subscribers are made within the ToolsTalk 2 application. All affected controllers will show the Push indicator in the Plant structure workspace.

Relevant Information

- Pushing Configurations to a Controller