# Configuring the ST Selector

The ST Selector is a tool accessory. It is installed on the tool and connected to the tool accessory bus. It has a small display, two input buttons and output LEDs.

1. Select a controller in the Plant structure workspace .

2. Select the Configurations icon in the top-side menu bar in the workspace area.

   The workspace area displays a list of configurations.

3. Double-click on a configuration row that has Tool configuration in the Type column.

   Alternatively, select the Add command button to create a new configuration.

   The workspace shows all the tool configuration menus.

4. Double-click on the ST selector in the Accessory bus menu, to open a shortcut window for the configuration.

5. Make the selected configurations. The configurations are auto-saved in ToolsTalk 2.

## Display

The display can show one piece of information at a time and has five different messages that roll in the display with a configurable display time.

ST selector display.
Parameter | Description
--- | ---
Switch time | Select the time to display one message before the next message is displayed.
Page | For each page 1-4, select a message from the shortcut menu that is to appear in the display for the duration of the switch time.

## Buttons

The two buttons can be configured to act upon the displayed information and can be used to step through the listed items.

ST selector buttons
Parameter | Description
--- | ---
Left button | Select one action from the shortcut menu.
Right button | Select one action from the shortcut menu.

## Status LEDs

The status LEDs can be activated or deactivated.

ST selector status LEDs
Parameter | Description
--- | ---
Enable result LEDs | Select the desired On or Off radio button.
Enable extra LEDs | Select the desired On or Off radio button.

The result LEDs which are red, green and yellow, show the same information as the main tools LEDs.

The two extra LEDs can show Batch OK and Batch sequence OK. Both these LEDs are automatically turned off at the next tightening.