# Revision History

ToolsTalk 2 Software version | Revision Date | Changes
--- | --- | ---
2.26 | 12/2025 | UPDATED content Prerequisites for Installation Compatibility Matrix Installation Overview Upgrading ToolsTalk 2 Installation Conditions Upgrading Process Description Installing the Client Application Installing the Client by Using ServerClickOnce NEW content Activated Joint Id - 225 Joint Id Result - 31046
2.25 | 04/2025 | UPDATED content Event Codes Open End in Open Position - 89 Updating Controller Software Working with the Virtual Station Tab Controller Fieldbus Mapping a Signal Configuration to One or More Virtual Fieldbuses Creating a Virtual Fieldbus Upgrading ToolsTalk 2 Prerequisites for Installation Compatibility Matrix Approval Statuses Fieldbus Sizes NEW content Ready to Operate For the Step Monitors page for Power Focus 6000 and Power Focus 8 and the Step Monitors page for FlexSystem and Synchronized tightening, the following steps are added: AZP - Adjust to Zero Position BA - Backlash Angle BM - Backlash Angle Measurement ZC - Zero Crossing
2.24 | 10/2024 | UPDATED content Working with the System Administration Tab: removed "External Links". Prerequisites for Installation and Installing the ToolsTalk Server Application: ports 22 and 80 can be changed during installation. The list of ports is updated. Information on how to enable HTTPS is added. To install ToolsTalk 2 version 2.24, .NET 8 is now required. Changes are made in Installation Overview, Prerequisites for Installation, and Installation Conditions. Some terms are changed, especially regarding "dual transducer" and to how transducers are referred. For example, instead of "primary angle" and "secondary angle", we now use "Angle" and "Angle 2", respectively. Upgrading ToolsTalk 2 contains all information about upgrade paths. The information was previously found in two different pages. Upgrading Process Description contains clarifications regarding versions, the Installation Configurator, and HTTPS-related settings that were introduced with ToolsTalk 2 v2.24 (Enable HTTPS and Server Authentication Certificate). Compatibility Matrix is updated with version 2.24 information. Installing the Client Application is updated with Enable HTTPS information. Installing the Client by Using ServerClickOnce is updated with Enable HTTPS information. NEW content Cyber Security Security List of Third-Party Licenses Controller Fieldbus For the Configuration for PF6000 and PF8 section, the following pages are added: Controller Fieldbus Prerequisites to Using Controller Fieldbus Creating a Controller Fieldbus Configuration Creating a Signal Configuration in the Controller Fieldbus Creating a Virtual Fieldbus Mapping a Signal Configuration to One or More Virtual Fieldbuses Mapping a Virtual Station to a Virtual Fieldbus Changing the Controller Offset For the Configuration for FlexSystem and Synchronized tightening section, the following pages are added: Controller Fieldbus Prerequisites to Using Controller Fieldbus Creating a Controller Fieldbus Configuration Creating a Signal Configuration in the Controller Fieldbus Creating a Virtual Fieldbus Mapping a Signal Configuration to One or More Virtual Fieldbuses Mapping a Virtual Station to a Virtual Fieldbus Changing the Controller Offset
2.22 | 03/2024 | UPDATED content Installing the Client by Using ServerClickOnceupdated regarding certificates Acyclic Result Itemsupdated with more detailded information Controller is Not Connecting to ToolsTalk 2updated Known InstallShield issueis the new title of the old section called Known Issues FMS - Uninstalling. Minor changes done in text. ToolsTalk Server does not Startupdated Logs to Include in Support Issuesupdated Installing the Station Setup Applicationupdated Handling Resultsupdated Controllersupdated with a new controller symbol Copying and pasting for tightening program updated in several sections of the User Guide Copying and pasting tightening programs (Configuration for PF600 and PF8), Copying and Pasting tightening programs (Configuration for FlexSystem and Synchronized Tightening), Tightening Program Library - Copying and Pasting Reference link added about rules for exporting and importing in Importing a Tightening Program and Importing a Multistep Program Copying and pasting for Batch Sequences and Sources updated in several sections of the User Guide Copying and pasting Batch Sequences and Sources (Configuration for PF600 and PF8), Copying and Pasting Batch sequences, Sync modes and Sources (Configuration for FlexSystem and Synchronized Tightening), All occurences of gear ratio changed to 100. All occurences of StepSync changed to Synchronized tightening or controller as applicable. NEW content Stopping error codesadded to Reference section. DELETED content Installation Pre-Requisites removed Known Upgrade Issues with Different ToolsTalk2 version removed ToolsTalk 2.13.4 with Atlas Copco Data Communication removed Toolstalk server does not Write to the Database ToolsTalk 2 is Not Connecting to Atlas Copco Data Communication Limitations
2.21 | 06/2023 | UPDATED content Migration to .NET6 done Changes done in Program Approval ToolsControl supported NEW content Upgrading ToolsTalk 2 from 2.20 to 2.21 added in Toolstalk 2 Installation and upgrade DELETED content The chapter "Enabling Microsoft MSMQ Server" removed and other information regarding MSMQ removed.
2.20 | 01/2023 | UPDATED content: Licences overview updated. Functionality Management System Definitions updated. The copy and paste instructions for Tightening programs, Batch sequences, Source Batch/Source Tightening and Sync modes replaced by a general instruction for Copy and Paste in TT2. Links and reference updated in RabbitMQ Overview. Installing OpenJDK made external Event codes updated
2.19 | 06/2022 | UPDATED content: Several limitations for StepSync are removed. General software improvements
2.18 | 01/2022 | NEW content: In multistep: Program Monitor: Time Program Restriction: Angle and Time In multistep: Step Type: Torque Calibration Step Monitor: Current and Torque Calibration. Step Restriction: Current. Extended logging Remote logging Open end configuration for PF6000 and PF8. Custom section folder implemented in Functionality Management System. IXB Tool Configuration - Vibrator New signals UPDATED content: General software improvements
2.17.1 | 09/2021 | NEW content: PF8 controllers are supported. Managing External links in System Administration tab. More filtering options in Tightening program tab. Possibility to delete the old configuration files when exporting controller configuration. More filtering options in Results tab. Information for RabbitMQ is added. UPDATED content: General software improvements
2.17 | 06/2021 | NEW content: PF6000 I/O Hub device is supported. Possible to export program details to .csv format from Controller tab, System Administration tab and Library tab. In multistep, more hold conditions are supported for Step Wait. In multistep, angle control processes is added for Step Restriction RT. In multistep for StepSync, signal for wait type is supported for SteySync. In multistep for StepSync, parameter Angle Window is added for Step Restriction RH. FlexSystem I/O Hub device is supported. Step Wait: Signal is supported for wait type. More hold conditions are supported. Optional parameter Program Start is added in Tightening Program Properties. Parameter Angle Window is added for Step Restriction RH. Angle control processes is added for Step Restriction RT. UPDATED content: Validating the ACDC Exchange Server Settings using a Server client and ClickOnce Server client Signal lists Event code list General software improvements DELETED content: Four step tightening strategy

Relevant Information

- Working with synchronized tightening