# Pushing Configurations to a Controller

WARNING

Risk of injury

A change in the configuration of the tightening program may cause unexpected torque, rotational direction, or speed in the system(s) where the tightening program is currently in use. This could result in severe bodily injury and/or property damage.

- Check the tightening program configurations after adding a new program or after applying changes to an existing program.

Pushing Configurations to One or More Controllers:

1. There are several different ways to push changes to a controller:

   - Select the Push indicator icon next to the controller name in the controller list.

   - Select the Manage button in the tab menu, then Push changes from the drop-down list.

   - Select the Push Changes button in the upper information bar.

2. After selection, the Controllers to push dialog window appears.

3. There are optional ways to push the configurations:

   A | Select this check box in order to push all configurations at once. This will apply to all controllers in the list.
   B | All configurations for the selected controllers will be pushed. Select controllers by marking the corresponding check box.
   C | Expand the list of configurations for a controller and handpick what configurations to be pushed. The remaining configurations will still be in the list after the selected ones have been pushed.

4. Select the Push command button (D).

5. Select Cancel or close the window to exit.