# Time Monitoring

Time monitoring is available for most tightening strategies, but has some variations:

- Time monitoring is not available for the Rotate strategy.

- Time monitoring is available for the Rundown stage.

- Time monitoring is available for the Final tightening step of the tightening stage.

- Time monitoring is used in conjunction with angle monitoring. When angle monitoring is enabled or the final target is an angle value, time monitoring is available.

If the time limits are violated during either stage, the tightening is terminated. The NOK detailed reason result is set accordingly.

In this Section

- Detailed NOK reason