# General Virtual Station

Adding a General Virtual Station

1. In the Plant structure workspace , select a controller.

2. In the tab menu bar in the workspace area, select the Configurations icon .

   The workspace area displays a list of configurations.

3. Double-click on a configuration row that has General Virtual Station in the Type column.

   Alternatively, select Add to create a new General Virtual Station configuration .

Properties
Parameter | Description
--- | ---
Name | Optional name for the configuration
Description | Optional configuration description

The non-tightening results can either be reported unfiltered (default), or configured to report a selection of the results. Up to 16 General Virtual Station configurations can be created.

Non-tightening results affected:

- Loosening

- Batch increment

- Batch decrement

- Reset batch

- Bypass tightening program

- Abort batch sequence

- Abort not started sequence

- Reset batch sequence

Relevant Information

- Assigning a General Virtual Station Configuration
- Global Configurations Library - Creating a Global Configuration From An Existing
- Pushing Configurations to a Controller
- Working with the Configurations Tab

In this Section

- Enabling and Disabling the Tightening Settings
- Configuring Live Result Settings