# Fieldbus Configuration Library - Creating or Importing a Global Fieldbus Configuration

## Creating a Fieldbus Configuration:

1. Select Library in the left-side menu bar.

2. Go to Fieldbus library .

   The workspace shows a list of Fieldbus configurations.

3. To add a new fieldbus configuration to the list, select Add.

   The Create new fieldbus configuration dialog window is displayed.

4. Enter the following parameters to add a new fieldbus map:

   - Enter a Name

   - Enter Size to controller and Size from controller

   - Select Controller type and Controller software version for the device, from the shortcut menu.

5. Select Add in the shortcut window.

6. The configuration window for the added fieldbus configuration is displayed.

The fieldbus configuration is auto-saved to the fieldbus library.

## Importing an Already Existing Fieldbus Configuration:

1. Select Library in the left-side menu bar.

2. Go to Fieldbus library .

   The workspace shows a list of Fieldbus configurations.

3. To add a new configuration to the list, select Add.

   The Create new fieldbus configuration dialog window is displayed.

4. Select the Import tab.

5. Select Open file.

   A browser window opens for reading the import file.

6. Select the desired import file. The file must be in the format <fieldbus_configuration_name>.json. Select Open.

7. Select Add in the shortcut window.

8. The configuration window for the added fieldbus configuration is displayed.

The fieldbus configuration is auto-saved to the fieldbus library.

Relevant Information

- Creating a New Fieldbus Map