# Adding a New Batch to a Batch Sequence

1. In the Plant structure , select a controller from the list.

2. On the menu bar, select the Batch Sequence tab . The workspace displays a list of batch sequences.

3. Select the Add command button in the Sequence configuration menu. The To create a new Batch Sequence window opens.

4. Issue the Batch Sequence with a name, and then select ADD.

5. Select the relevant parameters in the Properties.

6. Select a Sync Mode for the batch in Sequence Configuration.

7. Enter the Batch Size (the number of tightenings the batch will consist of).

8. Enter an optional Identifier Number.

The new Batch Sequence will be issued the first free position in the sequence list. If there are no free slots it will be placed at the bottom of the list and assigned the lowest available index number. It is not possible to change the index number to rearrange the batch tightening order.