# Tool Configuration - Direction Switch

The Direction Switch on the tool can be configured to trigger one input signal when quickly switched from clockwise (CW) to counter clockwise (CCW) and back, or vice versa.

1. Select a controller in the Plant structure workspace .

2. Select the Configurations icon in the menu bar.

   The workspace area shows a list of all the current accessory configurations.

3. Double-click on the name of the selected Tool configuration.

4. In the Direction Switch field, select the required signal from the Input drop-down list.