# Common Area Overview

The first occupied area contains the following items:

- Multiple tightening result

- Batch sequence result

- Result notification

These items are "common" and are not specific to a bolt or a channel and contain the following parameters:

Parameter name | Description
--- | ---
Type | Value type of each item. Example: batch sequence result value, result notification or multiple tightening result value.
Offset | Item position in the byte array with acyclic data frames and is defined in bytes.
Size | Size in bytes. It is possible to configure this manually if the datatype is a string. If the datatype is not a string, the values are set automatically based on the data type.
Data type | Data type values. Example: String, Int8, Int16 and so on.
Name | Item name. Non editable.

Relevant Information

- Acyclic Result Items

In this Section

- Adding Acyclic Result Configuration in Common Area
- Deleting Acyclic Result Configuration from Common Area