# Events Menu

Events are operational states and other pieces of information, for example errors, reported to the operator. All events can be configured and have different severity.

Event type | Function
--- | ---
Display | Events can be informative and are displayed for a short duration of time on the controller screen.
Log | Events can be informative and are displayed for a short duration of time on the controller screen and are also written to the log file. These will be displayed in the Events tab.
Acknowledge | Events that must be acknowledged by the operator. To acknowledge an event, the operator must press a button on an accessory, tap the controller touch screen or acknowledge the event through the web-GUI.

The event configuration determines how every event signals is treated.

Controller settings - events

A | Events search window | B | Events list

All available events are listed in the chapter References. Events have two categories:

- Standard events are defined by Atlas Copco and are available in every deliverable.

- Custom events are implemented by Atlas Copco on customer request and are only valid and available for specific customers.

Relevant Information

- Pushing Configurations to a Controller

In this Section

- Event Configuration
- Adding Events to the Library