# Summary for ISO 6789-2:2017

A | Add notes button | B | End test button
C | Statistic parameters |  |

The table displays the results of each measurement sequence, the available parameters are:

- Xa [Nm]: target indicated, set or nominal value depending on the type and class of the torque tool.

- Xr [Nm]: mean reference value determined by the measurement device.

- as [%]: calculated relative measurement error of the torque tool for the calibration torque.

- W: relative expanded measurement uncertainty of the torque tool at the calibration torque.

- W': relative measurement uncertainty interval of the torque tool at the calibration torque.

Tap the Add notes button to add comments to the inspection.

Tap the End test button to exit the result summary and end the test.

To print the test report: on the upper-right corner of the Summary category, tap Print report.

## Applies to: