# Summary category for SPC

When the subgroup defined in the SPC configuration is completed, the Summary category opens.

If one or more rules are violated, the SPC rules check result opens, showing the status of the rules.

If no rule is violated, the SPC rules check result is not shown.

After the dialog box appears, tap the Summary category.

In the Summary page, the following information are shown:

A | Add button | B | Restart test button
C | Statistic parameters | D | Enabled rules

The Add button is shown only for the SPC dimensional

The shown statistic parameters are:

- X: it is the average value of the results of the Inspection.

- R: it is the range value according to ISO standard.

- S: saved values related to the subgroup size defined in inspection configuration.

Below the statistic parameters, the enabled rules and their status are indicated.

If the rule is marked in:

- green: the rule is passed.

- red: the rule is failed.

- grey: the number of values is not enough to calculate the rule.

If a rule is disabled, it is not shown in the list.

Refer to the paragraph SPC rules for the procedure to enable/disable the SPC rules.

To restart the test, tap Restart test. The statistics are reset, and in the Summary page the results of the last test are shown.

To exit the test: on the upper-right corner of the Summary category, tap End test.

If the batch is completed, after the End test is tapped, the test is closed without showing any Confirmation message.

If the batch is not completed or the batch is set to zero, after the End test is tapped, a Confirmation massage is displayed.

To print the test label: on the upper-right corner of the Summary category, tap Print label.

In the label, the following information are shown:

- Barcode related to the Tool ID.

- Tool ID

- Nominal value of the test (torque, angle or both)

- Location of the tool

- Test date

- Date of the next test

## Applies to: