# Trace Limit Offset

The Start final angle point is set in the program as a torque value. The torque value has an undefined angle, called Offset value. From the Start final angle point it is easy to determine an angle to Final torque. The tightening must hit Final torque between Low limit angle and High limit angle. The value in brackets is 'Start final angle' + the limit value.

Example, Low 70 (334,7), where 70 is the Low Limit (C), and (334,7) is the offset value + Low Limit value (B+C) .

A | Start final angle (torque value)
B | Offset
C | Low Limit (Low Limit+offset)
D | HighLimit (HighLimit+offset)