# Process

## Product

Used for:

- Finding information about a specific range of products or a particular product, one may be interested in.

Various search options can be applied optionally in order to narrow down the query, out of which some can be found when selecting the button Advanced report in the upper right corner. Otherwise, these options are hidden as per default.

Upon selecting a specific product, it is then possible to see the details of the product: Tightening, Barcodes, Generic results and PR information.

## Station

Used for:

- Listing all production processes within a specific area, or of even only one single station of the entire production. This supports the user to draw potential conclusions from production deficiencies and the related areas they take place in.

## Process Overview

Used for:

- Listing and identifying overall efficiency of each individual assembly process in the production environment (e.g. specific tightening within a particular product model). The user can compare efficiency of individual assembly processes between product model.

## Top NOK

Used for:

- Getting statistics about amount and rate of NOKs processes in the production. The statistics makes it possible to identify processes which come with high NOK rates.

## Equipment Top NOK

Used for:

- Getting statistics about amount and rate of NOKs processes in the production per equipment. The statistics makes it possible to, identify potential equipment with high NOK rates and investigate the reason behind this.

## Flaw Overview

Used for:

- Identifying the reasons why assembly processes fail in the production environment. The user can analyse the main reasons why processes fail through the reasons that were provided by operators.

## Production Overview

Used for:

- Identifying potential process issues in the production area by receiving an aggregated process NOK percentage for the individual production sections.

## First Time Yield

Used for:

- Finding how much waste a single station creates.

It lets you identify the stations which have the most waste within your plant and understand what causing these waste.

Upon selecting a specific station it is possible either to see a history of the FTY or the details of the station.

## Rolled Throughput Yield

Used for:

- Analyzing the performance of the production.

It lets you identify the sections which have the most waste within your plant and understand which stations are causing these waste.

Upon selecting a specific location it is possible either to see a history of the RTY of that location, the FTY or the details of the stations under that location.

## Cycle time(Station Utilization)

- TheCycle Time feature helps engineers in manufacturing and production teams to evaluate how evenly workloads are distributed across assembly lines. It also highlights potential bottlenecks in production, providing actionable insights to improve process flow and increase overall output. It enables customers to see the average time required to produce their products at each location.

## Cycle Time Station(Assembly Process Durations)

- TheCycle Time Stationfeature helps engineers in manufacturing and production teams to analyze how workloads are distributed across a station’s dedicated assembly processes. It highlights potential bottlenecks and provides actionable data to improve station flow, ultimately supporting higher production output. It enables customers to see the average time required to assemble specific processes (tightening, barcode or generic result) at each station.