# System Requirements

## Atlas Copco Data Communication Software Requirements

- RabbitMQ, see Configuring the Settings Tab, RabbitMQ Overview.

- .NET 10.0.7 runtime, .NET Desktop 10.0.7 runtime and ASP.NET Core 10.0.7 runtime. Note: ASP.NET Core 10.0.7 requires both 32 and 64 bit installations.

- When HTTPS is enabled for the ACDC Web API or when TLS is enabled for Power Focus 6000, a valid certificate needs to be installed on the application server and configured to be used in Installation Configurator. See Configuring the Settings Tab.

To use TLS 1.3, Atlas Copco Data Communication must run on Windows Server 2022 or later.

HTTPS is disabled by default. If HTTPS is selected without a valid certificate, ACDC WebAPI and ACDC DataCommunication services will fail to start.

## Atlas Copco Data Communication Server Software Requirements

- Windows server, see release notes for verified versions.

For help with installation of this software, see the official web pages of the respective software providers.

## Database Server Software Requirements

- Microsoft SQL Server 2019 or later

Ensure that SQL Server Agent is activated before installation. Activate the SQL Server Agent in Windows services.

For help with installation of the Database Server software, see the official web pages of the respective software providers.

## PowerMACS Installation Requirements

For installation requirements with PowerMacs, see the PowerMacs 4000 User Guide.

To enable JoiningProcess for Pmacs Programs, install and run PowerMacsProgramService.

Install the correct ToolsNet Program Manager on the server. Make sure the ToolsNet Program Manager version matches or is higher than the PM4000 ToolsTalk version used to create the program.