# Operating the drill

WARNING

Crushing Hazard

Keep a safe distance from the tool during operation. A rotating tool can cause severe bodily injury.

- Make sure no body parts are near the tool during operation.

You can operate the drill as follows:

To quickly advance the drill bit to the work surface... | push the rapid advance button (optional). Make sure to stop the drill bit at a safe distance from the work surface.
To start drilling... | push the start button.
To stop drilling and retract the spindle into the start position... | push the retract button.
To switch off the motor in case of emergency... | push the emergency stop button.
To reset the emergency stop and restore normal operation... | pull the emergency stop button. Disconnect the air hose, and then reconnect it to reset the air logic.