# 3 Bending, Fig. B

Heat the spot to red colour.

It is recommended to concentrate the heat to the inside radius in order not to reduce the original width (W), see fig. B.

- After bending, allow to cool slightly in room temperature and then chill.

After bending, attach the accompanying warning sign to the reaction bar, see fig. C, and mark the side of the reaction bar that should be placed against the support in a suitable way.