# Air Pressure Monitoring, RE-signal

It is possible to connect the tool to a pressure monitoring equipment to monitor the tightening. The pressure signal from the tool (differential pressure over the motor) can be used to detect:

- Missed fasteners

- Trigger release before set torque is reached

- Stripped threads

- Cross-threading

- Re-hits

- Drop in air supply

To connect the tool to a pressure monitoring equipment we recommend using a Reporting Connection Kit, see Accessories https://servaid.atlascopco.com.

The pressure monitoring equipment does not measure torque.

## Assembly of the Reporting Connection Kit

## Air Pressure Signal Diagram