# Setting the Area Priority

The priority setting defines which tightening program should be selected if more than one area is active simultaneously.

- On the Edit Area screen, select Priority.

- Enter the priority number and then select OK

A higher number is prioritized over a lower number. 10 has priority over 1.

Relevant Information

- Changing the Name of an Area
- Creating a New Area
- Deleting an Area
- Editing an Area
- Setting Tool Distance Limits in an Area
- Setting Tool Orientation Limits in an Area