# General Mounting Directions

For optimal performance, mount the ILT Base Station with the list below in mind

- Do not place the ILT Base Station behind a metal object.

- Place the ILT Base Station close to the center of the tethering zone.

- Place the ILT Base Station so that it can be viewed and operated.

Mount the ILT Base Station maximum 2 meters above the floor.
If mounted higher than 2 meters above the floor, use additional safety equipment (for example, a steel wire) to secure the ILT Base Station to a rigid object.